单词:

nested 嵌套的；as of yesterday 截至昨日;on-demand 按需分配;colon 冒号；macros 宏命令

简称：

ACF Appliance Configuration Framework

AIR Auto Image Replication

AS AutoSupport

ASAP Appliance Security Assurance Program

ATDD Acceptance Test Driver Development

BMC Board Management Controller

BME Bare Metal Environment 裸机环境

BMR Bare Metal Restore

BnR Backup and Recovery

BSI Breakthrough System Inc.

CDS Cross-platform Data Sharing

CFT Critical Customer Escalations

CI Continuous Integration

CLISH Command Line Interface SHell/CISCO-like shell

CPI Common Product Installer

CR Content Router

A service that stores and retrieves file content. PureDisk breaks larger files into segments and distributes the segments across the available content routers.

DAR Direct Access Restore

DAS Direct Access Storage/Direct-attached storage

DG disk group

DHCP Dynamic Host Configuration Protocol

DOD Definition of Done

DRB Design Review Board

DR Site Disaster Recovery Site

EBOD Enterprise JBODs/Extended Bunch of Disks/Ethernet Connected JBOD

EEB Emergency Engineer Binary

EMM Enterprise Media Manager(a service)

EMW Enterprise Management Window

ET Etrack

FAT Fibre Accelerated Transport

FC fibre channel/​Feature Complete

FC-AL Fibre Channel arbitrated loop

FCL file change log

​FCoE Fibre Channel over Ethernet

FCR Fibre Channel Replication

FDD Feature Design Document

FQDN fully qualified domain name

FRU ​Field Replaceable Unit

FSM FT Service Manager

FT Fibre Transport

FTMS Fibre Transport Media Server

FSM Fibre Transport Service Manager

FYI for your infomation

GAB Group membership and Atomic Broadcast

GCO Global Cluster Option

GHS Global Hot Spares

GPT GUID Partition Table

HA High Available

HAD high availability daemon

HBA Host Bus Adapter

HCL Hardware Compatibility List

HW hardware

IaaS Infrastructure as a Service

IDF Innovation ...

IPFC IP over Fibre Channel

IPMI Intelligent Platform Management Interface​

IPS Innovation and Planning Sprint

IPS policy

I18N ​Internationalization

JBOD Just a Bunch of Disks

LBA Logical Block Address 逻辑块寻址

LLT Low Latency Transport

LSI

L10n ​Localization

MBR master root record

MLH

MSDP Media Server Deduplication Pool

MTV

NAS Network Attached Storage

NDMP Network Data Management Protocol

NEBS Network Equipment-Building System

NFR

N-port Node port

NUMA Non-uniform Memory Access

ODC Orthogonal Defect Classification

OOO Out of Office

OptDup Optimized Duplication

OSDO Open Storage Disk Option

Paas Platform as a Service

PBR Product Backlog Refinement

PCI

PD pure disk

PDA PureDisk Appliance

PDDE ​PureDisk Deduplication Engine

PDDO PureDisk deduplication option

A plug-in that uses the NetBackup OpenStorage API to enable NetBackup to write backups to a PureDisk storage pool.

All NetBackup data that is written to a PureDisk storage pool is deduplicated.

PI Product/Program Increment

PDFC (SAN based Replication)

PO Product Owner

POA Plan Of Action

POC Proof Of Concept

Potentially Shippable Product Increment 潜在的可交付产品增量

PTO Paid Time Off

PXE Preboot eXecution Environment与无人值守安装系统相关的

RAID Redundant Array of Inexpensive Disks

RBOD RAID bunch of Disks

RDMA remote direct memory access

RSM replicated state machine

RT Release Train

SaaS Software as a Service

SAFe ​Scaled Agile Framework

SAN Storage Area Network

SANBlaze

SAN Client

SBOD Switched Bunch of Disks

scale up adding more disks to a storage system

scale out grouping multiple systems together

SCL ​Software Compatibility List

SCST 一个驱动

SDCS Symantec Data Center Security

SDIO Velocity group

silver bullet

sisips 安装相关的做入侵检测控制的

SLP ​Storage Lifecycle Policy NBA做deduplication的policy

SMART Specific, Measurable, Attainable, Results-oriente, Time-delimited

SMcli Storage Manager Command Line Interface Utility

SMTP Simple Mail Transfer Protocol

SOA Service-Oriented Architecture

SP storage Processor

SPA Storage pool authority

The service that manages a storage pool.

SPAR storage pool authority replication

The replication of storage pool authority configuration information from an all-in-one local storage pool to a main storage pool.

SPAD Signaling Pathway Database

spoold the deduplication engine service

SRP SCSI RDMA Protocol

SSO Single Sign-On

STU Storage Unit

s/w

h/w

TMD Target Mode Driver

TCO total cost of ownership

Time Boxed 时间限制

TOI ​Transfer Of Information

UDID Unique Disk Identifier

UE User Experience

UMI Unique Message Identifier

VA Virtual Appliance

VCS Veritas Cluster Server​

VVA Velocity Virtual Appliance

VPA Velocity Physical Appliance

VPFS

VTO Virtual Tape Option

VxOS ​​Veritas Optimized Operating System

VxUL Veritas Unified Logging

VxVM Veritas Volume Manager

WWID worldwide id

WWN World Wide Name

WWNN Node WWN

WWPN Port WWN

ZRM zone\_reclaim\_mode

escalation是客服行业的术语，是一线客服解决不了的疑难问题就会escalate给专家座席或者叫二线客服，由他们来进行专业的处理。

kick-off开球、开始

recap 概况、扼要重述

phishing 网络钓鱼

follow up 把...探究到底，回答，跟进，追踪